> Connect Pano Manager To VirtualCenter
> The Pano Manager must be able to communicate with VirtualCenter in order to use the Pano Manager's connection brokering and automated deployment features.
> If you plan to use VMware View exclusively, then you do not need to perform this procedure (for more information, go to (Overview) Integrate Pano VDS with VMware View.
> To enable communication between Pano Manager and VirtualCenter:
> Before You Begin: Prepare To Integrate Pano Manager

> 1. | Ensure that VirtualCenter web service is installed and running; otherwise, the Pano Manager can’t communicate with VirtualCenter. Go to VMware’s “Verifying VirtualCenter Web Service Installation” procedure.

> 2. | Log on to the Pano Manager.

> 3. | Click the Setup tab.

> 4. | In the Virtualization Configuration area, type the URL for the VirtualCenter interface. The URL can be a FQDN of the computer, IP address, or Netbios name. As long as the URL can resolve to the IP address, it will work.

> For VirtualCenter 2.x:

> http[s]://host/sdk

> Example:

> https://vcserver/sdk

> 5. | Type the user name of the account in VMware VirtualCenter.

> The Pano Manager uses this account to communicate with VirtualCenter. It is recommended that this account be unique–and only used for integration between the Pano Manager and VirtualCenter. The username must be a valid user who has permissions on the Folder hierarchy in VirtualCenter as well as customization scripts and other objects.

> 6. | Type the account's password, then click Configure.

> 7. | When connected, In the Virtualization Configuration area, click Browse, then browse the virtualization hierarchy to confirm that the account has the proper access privileges.

> Troubleshooting: Troubleshoot Communication Problems with VirtualCenter
> Next Step(s): Choose a Pano Device Discovery Method

Did you find what you're looking for?
v2.5.1