> Normal Login Process
> Once a Pano device is connected to a Pano Manager, the Pano client login screen is displayed to the user. After the user enters the username and password and hits the Login button, the Pano Manager displays the user's desktop.
> Between the time the user hits the Login button and the desktop is displayed, the screen turns blank and the color on the Pano Button changes to solid orange for a few seconds. This sequence exists because the Pano Manager transfers the connection of the Pano device to the Pano Desktop Service (Pano DAS) running on the DVM.
> There is a small interval of time between which the connection of the Pano device to Pano software (Pano software refers to Pano Manager or Pano DAS) is broken. This is normal behavior and the disconnection should only last a couple of seconds.

Did you find what you're looking for?
v2.5.1