> What’s the maximum power that a Pano device can draw?
> A Pano device has 3 USB ports. The USB specification is 500mA @ 5V per port. The Pano device’s meets this USB specification for RevB-03 and RevB-02. RevC supports up to 700mA.
> However, you are only allowed 2 high power (500mA) USB devices and 1 low power (100mA) USB device at one time on a Pano device.

Did you find what you're looking for?
v2.5.1