> Configure Data Center Firewall
> The Pano DAS communicates with the Pano Manager and Pano devices over certain network ports. If you have a firewall between your users Pano devices and your data center, you must open up these ports for both inbound and outbound traffic. DVMs initiate connections to Pano devices, not the other way around. If these ports are closed, Pano Manager cannot discovery your Pano devices.
> Next Step(s): Connect Pano Manager To Directory Services

Did you find what you're looking for?
v2.5.1