> Pano Manager Network Port Usage
> The components of Pano VDS, Pano Manager, Pano Desktop Service and Pano Device, communicate with each other on several ports. In order to function properly, these components require access to these ports. So, you must open these ports and adjust firewall rules accordingly.
> Apart from Inbound ports used and Outbound ports used on the Pano Manager, you also need to specify the ports used between Pano devices and the Pano DAS.
> For more information, go to Configure DVM Firewall and Configure Data Center Firewall.

> • | Inbound Ports Used by Pano Manager

> Ports | Protocol | Service | Usage
> ICMP |  | ping | Test connectivity to the server
> 80 | TCP | HTTP | Connections from the UI to control the Pano Manager
> 443 | TCP | HTTPS | Connections from the UI to control the Pano Manager
> 22 | TCP | SSH | Remote terminal access
> 68 | UDP | DHCP | DHCP responses
> 123 | UDP | NTP | Synchronizing of server time
> 8320 | UDP |  | Communication from the Pano
> 8321 | UDP |  | Communication from the Pano

> • | Outbound Ports Used by Pano Manager

> Ports | Protocol | Service | Usage
> ICMP |  | ping | Test connectivity to the server
> 53 | TCP | DNS | DNS requests
> 80 | TCP |  | Communication to VirtualCenter
> 443 | TCP |  | SSL communication to VirtualCenter
> 389 | TCP | LDAP | Communication to LDAP server
> 636 | TCP | LDAPS | Communication to LDAP server (Secured)
> 3268 | TCP |  | Communication to the Global Catalog
> 3269 | TCP |  | Communication to the Global Catalog (Secured)
> 8319 | TCP |  | Connection brokering to the Pano devices
> 53 | UDP | DNS | DNS requests
> 67 | UDP | DHCP | DHCP
> 123 | UDP | NTP |
> 389 | UDP | LDAP | Communication to LDAP server
> 636 | UDP | LDAPS | Communication to LDAP server (Secured)
> 8321 | UDP |  | Connection brokering to the Pano devices

> • | Inbound Ports Used by Pano DAS

> Ports | Protocol | Service | Usage
> 8319 | TCP |  | Communication from the Pano Manager to the Pano DAS
> 8321 | UDP |  | Communication from the Pano Manager to the Pano devices

> • | Outbound Ports Used by Pano Devices

> Ports | Protocol | Service | Usage
> 8320 | UDP |  | Communication from a Pano device to the Pano Manager
> 8321 | UDP |  | Bi-directional communication to/from the Pano Manager

Did you find what you're looking for?
v2.5.1