> Configure Pano Manager VM Network Settings
> You can configure the Pano Manager VM (Pano Manager VM) to get its network settings from a DHCP Server or you can assign the Pano Manager VM a static IP Address. Setting a static IP address is generally preferred, and is required if you use DHCP-assisted discovery for Pano device as outlined in (DHCP Method) Set Up Pano Device Discovery.
> To configure the Pano Manager VM’s network settings:

> 1. | Power on the Pano Manager, if not already.

> 2. | Log on to Pano Manager VM.

> 3. | Select option 1. The Use DHCP (y/n)? prompt appears.

> 4. | Specify the network settings for the Pano Manager VM. Set to DHCP or provide static IP.

> Next Step(s): Do the following:

> 1. | If you want to upload a self-signed certificate, go to (Overview) Replace Pano Manager’s Self-Signed Certificate

> 2. | If you’re performing this task as part of a deployment, return to (Start Here) Deploy Pano VDS to determine the next step.

Did you find what you're looking for?
v2.5.1