> About Pano Devices Tab

> Column Name | Description
> Name | The name of the Pano device. The Pano Manager automatically generates this name. You can edit the name by clicking on the Edit... button.
> Secondary | The Pano device associated with the Pano device that shows the secondary monitor for the user.
> Dual Monitor | Lists the association between Pano devices.
> MAC Address | The unique MAC address for the Pano device's network interface.
> IP Address | The IP Address of the Pano device.
> Connection | Connection status of the Pano device as known to the Pano Manager. The status can be:
> • | Unreachable - The Pano Manager cannot contact the Pano device.
> • | Discovered - The Pano Manager has discovered the Pano device on the network.
> • | Login - The Pano Manager is running the login screen and is waiting for a user to log on.
> • | DVM - The DVM is connected to a Pano Manager.
> Rx Packets | Number of packets per second received by the Pano device as observed by the Pano DAS.
> Re Rx Packets | Number of identical packets per second received by the Pano device multiple times as observed by the Pano DAS.
> Tx Packets | Number of packets per second transmitted by the Pano device as observed by the Pano DAS.
> Re Tx Packets | Number of identical packets per second transmitted by the Pano device multiple times as observed by the Pano DAS.
> Min RTT | Minimum round-trip time from the Pano device to an agent on the DVM and back. A “normal” range varies from network to network; compare this metric against typical traffic for your specific network.
> Avg RTT | Average round-trip time from the Pano device to an agent on the DVM and back. A “normal” range varies from network to network; compare this metric against typical traffic for your specific network.
> Max RTT | Maximum round-trip time from the Pano device to an agent on the DVM and back. A “normal” range varies from network to network; compare this metric against typical traffic for your specific network.

Did you find what you're looking for?
v2.5.1