> How many IP addresses do I need to run Pano VDS?
> Your Pano Virtual Desktop Solution is meant to be efficient and to merge easily into your existing network infrastructure. For the Pano Manager itself you'll only need one additional static IP in addition to the IP(s) that are already used by your VMware host. The Pano devices themselves get their IP addresses from your DHCP server, just as any other PC or network device would in most networks.

Did you find what you're looking for?
v2.5.1