> Add Pano Logic Vendor Class for Netware DHCP Server
> Here is an example of a configuration for a Netware DHCP server:
> Where the value of option 43 must be in hex format (for example, 01040ADC641D):

> • | The first byte (01) is the code.

> • | The second byte (04) is the length.

> • | The remaining bytes comprise the IP address of the Pano Manager after it has been converted to hex format (for example, 182.21.5709 converts to 0ADC641D). Use this tool to convert the IP address to hex.

> For more information, go to Using DHCP option 43 (Vendor Extensions).

Did you find what you're looking for?
v2.5.1