> What are the bandwidth requirements for Pano VDS?
> Bandwidth consumption is always a variable just as with a normal PC depending on if you're running at idle or doing things that cause bursts of traffic. Pano VDS is typically very minimal on network overhead and on average only consumes around 150kbps per Pano device. For overall bandwidth requirements, go to Hardware and Resource Requirements.
> This consumption will continue to decrease with forthcoming revisions of the Pano hardware/software so that you'll get maximum performance with the least bandwidth possible in both the LAN and WAN implementations.

Did you find what you're looking for?
v2.5.1