> Are the screenbits encrypted between the Pano device and its associated DVM?
> Keyboard and mouse traffic are encrypted between Pano devices and ESX server. Such encryption prevents anyone from being able to piggy back onto the network using packet sniffers. However the screen traffic is not encrypted, as the screen traffic is binary and represents just screen bits.

Did you find what you're looking for?
v2.5.1