> Add Pano Logic Vendor Class for Cisco IOS DHCP Server
> From your Cisco IOS CLI you need to specify the configuration mode, create a pool, and set a pool name for your Pano devices. You also need to set proper options.
> Here is an example of a configuration for a Cisco IOS DHCP server.

> ip dhcp pool PoolName option 66 ascii "Pano Logic" option 60 ascii "PXEClient" option 43 hex 01:04:AC:13:35:17

> Where the value of option 43 must be in hex format (for example, 01:04:AC:13:35:17):

> • | The first byte (01) is the code.

> • | The second byte (04) is the length.

> • | The remaining bytes comprise the IP address of the Pano Manager after it has been converted to hex format (for example, 172.19.53.23 converts to AC:13:35:17). Use this tool to convert the IP address to hex.

Did you find what you're looking for?
v2.5.1