> (RDP Connections Only) Configure Pano DAS for 24‑bit Color
> 16-bit uses less network bandwidth and gives your users better responsiveness; 24-bit gives richer and smoother color, but is a bit more network intensive.
> When connecting to a DVM via Remote Desktop Connection or the Pano web access, you must configure the DVM if your users desire 24-bit color depth.
> By default, your Pano devices use 16-bit color depth and you don't need to configure anything. However, if you want your Pano devices to use 24-bit color depth, you must configure Pano Desktop Service (Pano DAS) by editing the DVM’s registry.
> Warning: If you use Registry Editor incorrectly, you can cause serious problems that can require you to reinstall your operating system. Neither Pano Logic nor Microsoft can guarantee that you can solve problems that result from using Registry Editor incorrectly. Use Registry Editor at your own risk.
> To configure Pano DAS for 24-bit color depth:
> After you perform this procedure and the next time you log on to the DVM through a Pano device, you get 24-bit color depth. If you choose to use 16-bit color depth in the future, you can simply change the value of the registry to 16.
> Warning: If you choose to configure your virtual machine to support up to 16‑bit color only, you must change the value of the registry entry you’re about to create to 16 or delete the registry. Otherwise, you won't be able to log on to the virtual machine from a Pano device.

> 1. | Launch the Registry Editor:

> a. | From Windows, click Start > Run

> b. | Type regedit, then click OK.

> 2. | Navigate to HKEY_LOCAL_MACHINE\Software\Pano Logic, Inc.\Pano Desktop Additions.

> 3. | Add a string entry Pixel Bit Depth, and set its value to 24.

> 4. | Restart the Pano Desktop Additions service or reboot your desktop virtual machine.

Did you find what you're looking for?
v2.5.1