> Configure Pano DAS for 24-bit Color
> 16-bit uses less network bandwidth and gives your users better responsiveness; 24-bit gives richer and smoother color, but is a bit more network intensive.
> When connecting to a DVM via Remote Desktop Connection or Pano web access, you must configure the DVM if your users desire 24-bit color depth. To do so, go to (RDP Connections Only) Configure Pano DAS for 24‑bit Color.
> When connecting via a Pano device to a DVM with Console Direct, your users can select 16‑bit or 24‑bit color depth through the Pano Control Panel. No other configuration is required.
> To select 24‑bit color depth from the Pano Control Panel:

> 1. | From the Pano Control Panel, click the Display tab.

> 2. | In the Color quality drop-down, choose 24 bits.

Did you find what you're looking for?
v2.5.1