> Configure Pano Devices for Dual‑Monitor Use
> Two Pano devices can be configured to work as a team to provide a single Windows desktop that is spanned across two monitors. To configure this option attach two Pano devices to the network as normal. Make sure each Pano device is discovered by the Pano Manager and that you can access the Pano VDS from either device.
> The requirements for dual-monitor use are as follows:

> • | The primary monitor must be placed to the left of the secondary monitor.

> • | The monitors that make up the pair must support a common vertical resolution.

> • | Both Pano devices must be attached to the network and functioning. This pair of Pano devices operate as a team. If any member of the team is not available you will not be able to log on.

> To configure a pair of Pano devices for dual-monitor use:

> 1. | Arrange the equipment so that the Pano device that is to be primary is connected to the left monitor and the Pano device that is to be the secondary is connected to the right monitor.

> 2. | Log on to the Pano Manager.

> 3. | Click on the Pano devices tab.

> 4. | Select the primary Pano device from the list and click Edit….

> 5. | Type the name of the secondary Pano device.

> You can type in the name of the device, or use the browser to choose from a list of available devices.

> 6. | Click Update Pano Device.

> To change to a single monitor configuration, simply edit the properties of the primary Pano device and delete the information in the Secondary Monitor field.

Did you find what you're looking for?
v2.5.1