> How do Pano devices get IP addresses?
> Your Pano devices get their IP addresses from your DHCP server. There is no facility or need to configure an IP address directly on a Pano device. Just plug it in!
> If you need to assign a specific IP address, you can easily do so by reserving specific IP addresses within your DHCP IP address pool(s); however, each Pano device must get its address from your DHCP server, and each IP address must be unique.

Did you find what you're looking for?
v2.5.1