> Verify Newly Created DVMs
> The key aspects of verifying a newly created DVM includes ensuring that the DVM appears in the Pano Manager, and that the Pano DAS is running.
> To verify a newly created DVM:

> 1. | Log on to the Pano Manager.

> 2. | Click the DVM tab, verify that everything looks okay.

> | Verify... | Field/Value
> | The DVM appears in the table. | Virtual Machine Name
> | The DMV is powered on. | DVM State indicates PoweredOn
> | The DVM has an IP address that was acquired using DHCP | IP Address and DNS Name have appropriate values
> | The Pano Desktop Service (Pano DAS) is running and responding to status check messages from Pano Manager. | DAS Status indicates Responding
> | The version of Pano DAS appears, and is the expected version. | DAS Version
> | The desktop virtual machine shows a user in the field, if you created User Based Collections. If not, that’s because you forgot to add users. You can do so now. Go to Assign Pano Devices and Users To DVMs. | Assigned User
> | The desktop virtual machine shows a user logged on. If not, log on using that user’s DVM to ensure that you can connect. | Logged In User
> | The desktop virtual machine shows clients connected, if you created Device Based Collections. If not, no Pano device is connected to this DVM. Connect via a Pano device to make sure it’s working. | Client

> 3. | Click the Pano device tab, and verify that everything looks okay.

> | Verify... | Field/Value
> | The login screen is being displayed on the monitor that is connected to the Pano device. | Connection indicates DVM or Pano device is connected to a DVM
> | The Pano device has a MAC address and IP address | MAC Address and IP Address
> | The Pano device is assigned to the DVM. | Assignment

Did you find what you're looking for?
v2.5.1