> Manually Add Pano Devices
> If you enabled one of the following automatic discovery methods during setup, Pano Device discovery automatically discovers and adds the Pano devices to your Pano Manager:

> • | (Broadcast/Probe Method) Set Up Pano Device Discovery

> • | (DHCP Method) Set Up Pano Device Discovery

> If you do not enable one of theses discovery methods, then you need to manually add Pano devices. Pano Logic recommends that you use a discovery method. The only reason to manually add Pano devices is if you have more than one Pano Manager in your environment, and this configuration is very unusual.
> To manually add a Pano device:

> 1. | Log on to the Pano Manager.

> 2. | Click on the Pano devices tab.

> 3. | Click Add.

> 4. | Type the name you want to use to identify the Pano device. For example, you can enter a user name or the physical location of the Pano device.

> 5. | Type the MAC address of the Pano device.

> 6. | Type the IP address.

> 7. | Click Add Pano.

Did you find what you're looking for?
v2.5.1