> Why can’t I find my Pano devices, even though I’ve defined a vendor class in my DHCP server?
> Do the following:

> • | Verify that vendor class is properly configured, and that your dhcp service or daemon is running.

> • | Check your networking and firewall settings: verify that necessary communication ports aren’t being blocked. For more information, go to Firewall prevents communication.

Did you find what you're looking for?
v2.5.1